[bookmark: _vcvtdf4p4c1]01_CDL_Master 120-Day Curriculum Blueprint
[bookmark: _qase8b2xus4c]Section 1: Federal ELDT Compliance Framework & Program Overview
The  CDL Class A Esports Training Program  is a 120-day master curriculum designed to transition candidates from gaming environments to commercial driver's license (CDL) holders and remote Tesla Semi teleoperators. The program is built around the Federal Motor Carrier Safety Administration (FMCSA) Entry-Level Driver Training (ELDT) regulations effective as of February 7, 2022 (governed by 49 CFR Part 380, Subparts F and G, along with Appendices A through E).
[bookmark: _rit531f9t6c7]Regulatory Requirements & Training Provider Registry (TPR)
· Theory Instruction Mandate : Covers all 30 mandated FMCSA ELDT theory topics across 5 primary categories. Federal regulations set no minimum hour threshold for theory; however, candidates must achieve a minimum score of  80% or higher  on comprehensive theory assessments.
· Behind-the-Wheel (BTW) Instruction Mandate : Requires separate Range and Public Road instruction delivered in a physical Commercial Motor Vehicle (CMV) by an eligible provider. BTW training is proficiency-based (with logged hours reported separately) and requires candidates to demonstrate mastery in pre/post-trip inspections, basic vehicle control, backing maneuvers, and public road operations (urban, rural, highway, night).
· Reporting Deadlines : Qualifying theory and BTW completions must be transmitted to the FMCSA Training Provider Registry (TPR) by midnight of the second business day following program completion. Completion must be submitted prior to the candidate taking the state CDL skills test.
· Prerequisites : Commercial Learner's Permit (CLP) holding, valid DOT medical certification, and age requirements (minimum 18 for intrastate, 21 for interstate operations).
[bookmark: _lswvv6fkpypo]Enrollment & Compliance Architecture
1. Intake & Screening : Initial eligibility verification, exception screening, and background/medical qualification.
2. CLP Preparation & Registered Theory : Virtual theory instruction supported by interactive gaming modules, virtual pre-trip inspections, hazard recognition simulations, and backing geometry drills.
3. Assessment & Verification : Versioned lesson tracking, instructor validation under 49 CFR 380.605, and achievement of the 80% minimum theory pass threshold.
4. TPR Reporting : Automated upload of theory completion records to the FMCSA TPR.
5. BTW Partner Integration : Transition to registered BTW partners for range maneuver logging and public road driving.
6. State Skills Examination : Final state-administered testing (Pre-Trip, Backing, Road Test) for CDL Class A issuance.
[bookmark: _lelxid2o5yoo]Section 2: 30 FMCSA ELDT Theory Topics & Esports Mapping Matrix
The curriculum integrates all 30 required ELDT theory topics into game drills, classroom modules, and simulation environments:| # | ELDT Theory Topic | Category | Mapped Esports Game Drill / Curriculum Module || ------ | ------ | ------ | ------ || 1 | Orientation | Basic Operation | Game 0: Orientation Sim || 2 | Control Systems / Dashboard | Basic Operation | Game 1: Dash Master || 3 | Pre/Post-Trip Inspections | Basic Operation | Game 3 (or Game 4 in chart): Inspection Hunt || 4 | Basic Control | Basic Operation | Game 0: Aim Lab Wheel || 5 | Shifting / Operating Transmissions | Basic Operation | Game 2: Shifter Module || 6 | Backing and Docking | Basic Operation | Game 2 (or Game 3 in chart): Backing Tetris || 7 | Coupling and Uncoupling | Basic Operation | Game 5: Coupling Chaos || 8 | Visual Search | Safe Operating Procedures | Game 1: Mirror Management || 9 | Communication | Safe Operating Procedures | Game 7: Comms Module || 10 | Distracted Driving | Safe Operating Procedures | Game 10: Signal Survival Remote CDL || 11 | Speed Management | Safe Operating Procedures | Haul Time Trial || 12 | Space Management | Safe Operating Procedures | Game 1: Mirror Management || 13 | Night Operation | Safe Operating Procedures | Night Ops Simulation || 14 | Extreme Driving Conditions | Safe Operating Procedures | Game 8: Skid Control / Recovery || 15 | Hazard Perception | Advanced Operating Practices | Game 7: Hazard Highway || 16 | Skid Control / Recovery / Jackknifing | Advanced Operating Practices | Game 8: Skid Recovery || 17 | Railroad-Highway Crossings | Advanced Operating Practices | Game 7: Hazard Highway || 18 | Identification & Diagnosis of Malfunctions | Vehicle Systems & Malfunctions | Dash Master / Remote Diagnostics || 19 | Roadside Inspections | Vehicle Systems & Malfunctions | Game 3: Inspection Hunt || 20 | Maintenance | Vehicle Systems & Malfunctions | Game 9: Tesla Battery Mgmt || 21 | Handling and Documenting Cargo | Non-Driving Activities | Game 4: Load Secure || 22 | Environmental Compliance | Non-Driving Activities | Game 11: Trip Planning Optimizer || 23 | Hours of Service (HOS) Requirements | Non-Driving Activities | Game 6: HOS Puzzle || 24 | Fatigue and Wellness | Non-Driving Activities | Wellness Sim Module || 25 | Post-Crash Procedures | Non-Driving Activities | Post-Crash Simulation || 26 | External Communications | Non-Driving Activities | Game 12: Fleet Manager Sim || 27 | Whistleblower / Coercion | Non-Driving Activities | Classroom Compliance Module || 28 | Trip Planning | Non-Driving Activities | Game 11: Trip Planning Optimizer || 29 | Drugs / Alcohol Regulations | Non-Driving Activities | Classroom Zero-Tolerance Module || 30 | Medical Requirements | Non-Driving Activities | DOT Medical Qualification Module |
[bookmark: _dm7nofsqn0gc]Section 3: Tesla Semi Technical Specifications & Remote Teleoperation Protocols
[bookmark: _hcm5i8jjfzw]Tesla Semi Hardware & Performance Profile (2026 Production)
· Vehicle Class : Class 8 Heavy-Duty Commercial Tractor.
· Powertrain : 3 independent electric motors generating ~1,070 hp (800 kW).
· Range & GCW : 500-mile long-range variant at 82,000 lbs Gross Combination Weight (GCW).
· Energy Consumption Target : 1.7 kWh per mile fully loaded.
· Payload Capacity : 48,000 lbs tractor payload.
· Charging Infrastructure : 1.2 MW Megacharger system.
· Cab Configuration : Central driving position with dual touchscreen displays.
· Sensor Suite & Telematics : Hardware 4 (HW4) with 8 external cameras, Over-the-Air (OTA) updates, remote diagnostics, and electric Power Take-Off (ePTO).
· Manufacturing Facility : Production volume originating out of Nevada (H1 2026).
   +-----------------------------------------------------------------+
   |                     TESLA SEMI SPECIFICATIONS                   |
   +-----------------------------------------------------------------+
   | Motors:           3 Electric Motors (~1070 hp / 800 kW)         |
   | Max Range:        500 Miles at 82,000 lbs GCW                    |
   | Target Efficiency: 1.7 kWh / Mile (Loaded)                      |
   | Charging Standard:1.2 MW Megacharger System                     |
   | Operator Seat:    Central Driving Position                      |
   | Camera Hardware:  HW4 Suite (8 Surround Cameras)                |
   | Payload Capacity: 48,000 lbs                                     |
   +-----------------------------------------------------------------+

[bookmark: _xmp2am6btc3i]Remote Teleoperation Protocols & CPUC Regulatory Framework
Based on California Public Utilities Commission (CPUC) filings (Feb 2026) and FMCSA guidelines, remote operators stationed in teleoperation centers (e.g., Austin, TX and Bay Area, CA) manage Level 2 FSD Supervised systems with a human-in-the-loop remote backup architecture.
[bookmark: _uaeh5svbgka2]Operator Qualification Requirements
1. Active US Class A CDL.
2. Background clearance and mandatory pre-employment/random drug & alcohol testing.
3. Teleoperation training certification covering multi-camera stream analysis and signal latency mitigation.
[bookmark: _b1owlltv6tuf]Technical Dynamics & Constraints
· Latency Thresholds : Teleoperation streams operate within a  100–400 ms latency  window. Training incorporates artificially induced packet loss, jitter, and camera feed freezes.
· Multi-Camera Management : Remote operators continuously monitor 24 feeds across 3 assigned vehicles (8 cameras per vehicle).
· Emergency Stop (E-Stop) Protocol : Mandatory trigger execution within  <0.8 seconds  upon detection of feed corruption, excessive latency (>400 ms), or unresolvable path obstacles.
[bookmark: _pvor9hqhbaik]Section 4: 120-Day Seasonal Curriculum Roadmap
+-----------------------------------------------------------------------------------+
|                        120-DAY CDL ESPORTS MASTER ROADMAP                         |
+-----------------------------------------------------------------------------------+
|  SEASON 1: Rookie Bootcamp (Days 1-30)   |  SEASON 2: Operator (Days 31-60)       |
|  - ELDT Theory: Topics 1-7               |  - ELDT Theory: Topics 8-14           |
|  - Focus: Basic Operation & CLP Prep     |  - Focus: Safe Ops & BTW Range        |
|  - Games: 00, 01, 02                     |  - Games: 03, 04, 05, 06              |
+------------------------------------------+----------------------------------------+
|  SEASON 3: Pro League (Days 61-90)       |  SEASON 4: Masters (Days 91-120)       |
|  - ELDT Theory: Topics 15-20             |  - ELDT Theory: Topics 21-30           |
|  - Focus: Advanced, Road & Tesla Semi    |  - Focus: Non-Driving & Remote Ops     |
|  - Games: 07, 08, 09, 10                 |  - Games: 11, 12, 13 (Capstone Finals) |
+-----------------------------------------------------------------------------------+

[bookmark: _9xfmylzc6qj0]Season 1: Rookie Bootcamp (Days 1–30) — Theory & Basic Control
· ELDT Theory Mapped : Topics 1–7 (Orientation, Dashboard, Pre/Post-Trip, Basic Control, Shifting, Backing, Coupling).
· Milestones : Medical Examiner's Certificate (DOT Medical), CLP test preparation, theory practice evaluations (80%+ threshold).
· BTW / Simulator Focus : Steering precision, inertia management, mirror scanning geometry.
· Game Drills : Game 00 (Aim Lab Wheel), Game 01 (Mirror Management), Game 02 (Backing Tetris).
· Competitive Event : Daily leaderboard challenges awarding XP for defect-free virtual pre-trip inspections.
[bookmark: _dok9dtmbsrk8]Season 2: Operator (Days 31–60) — Safe Ops & BTW Range
· ELDT Theory Mapped : Topics 8–14 (Visual Search, Communication, Distracted Driving, Speed Management, Space Management, Night Operations, Extreme Conditions).
· BTW Range Execution : Physical range maneuvers logged for proficiency: straight-line backing, offset backing, parallel parking, and 90-degree alley docking.
· Game Drills : Game 03 (Inspection Hunt), Game 04 (Load Secure), Game 05 (Coupling Chaos), Game 06 (HOS Puzzle).
· Competitive Event : Weekly 1v1 Backing Tournament in a bracket format using standardized dock seeds.
[bookmark: _5xu77esta38d]Season 3: Pro League (Days 61–90) — Advanced Ops, Public Road & Tesla Semi
· ELDT Theory Mapped : Topics 15–20 (Hazard Perception, Skid Control/Jackknifing, Railroad Crossings, Malfunction Diagnosis, Roadside Inspections, Maintenance).
· BTW Public Road Execution : Urban, rural, two-lane highway, interstate driving, and night driving proficiency logging.
· Tesla Semi Specialized Module : Central seat ergonomics, one-pedal regenerative braking control, battery range planning, 1.2 MW Megacharger stops, ePTO management.
· Game Drills : Game 07 (Hazard Highway), Game 08 (Skid Recovery), Game 09 (Tesla Battery Mgmt), Game 10 (Signal Survival Remote CDL).
· Competitive Event : Team Relay, Night Ops Cup, and Tesla Efficiency Challenges.
[bookmark: _pa08btin5fo0]Season 4: Masters (Days 91–120) — Non-Driving Activities, Teleoperation & Hiring
· ELDT Theory Mapped : Topics 21–30 (Cargo Handling, Environmental, HOS Rules, Fatigue/Wellness, Post-Crash, External Comms, Whistleblower, Trip Planning, Drugs/Alcohol, Medical Requirements).
· Remote Operator Training : Teleoperation compliance, background checks, signal redundancy, and Austin/Bay Area operations center workflows.
· Game Drills : Game 11 (Trip Planning Optimizer), Game 12 (Fleet Manager Sim), Game 13 (Rescue Relay CDL Capstone).
· Championship Event (Day 120) : Final 500-mile Tesla Semi Efficiency & Safety Championship. Carrier recruitment panels evaluate performance; top finishes generate automated GoHighLevel (GHL) CRM opportunity profiles.
[bookmark: _v3vhrpkt5252]Section 5: Specialized Esports Game Drills (Games 00–13)
[bookmark: _a3e3vvbf4xa6]Game 00: Aim Lab Wheel
· Description : Precision steering drill requiring candidates to guide a heavy vehicle wheel to 20 random targets while adjusting for steering rebound and weight inertia.
· ELDT Mapping : Basic Control, Control Systems / Dashboard.
· Scoring Metrics : Smoothness (0–100), Accuracy (0–100), Rebound Control.
[bookmark: _45avebwsq5t0]Game 01: Mirror Management
· Description : Candidates monitor 6 traditional convex/flat mirrors alongside 8 Tesla surround-camera feeds to detect rapidly emerging blind-spot hazards within a 3-second window.
· ELDT Mapping : Visual Search, Space Management, Communication.
· Scoring Metrics : Hazard Detection Rate (%), Mirror Check Frequency (checks/min), Visual Sweep Latency.
[bookmark: _117z17ads213]Game 02: Backing Tetris
· Description : Simulated backing maneuvers including 90-degree alley dock, offset back, and parallel parking. Candidates must center the trailer in a designated blueprint target zone within <10 cm margin of error.
· ELDT Mapping : Backing and Docking.
· Scoring Metrics : Final Placement Error (cm), Pull-Up Count, Get Out And Look (GOAL) Compliance, Zero Boundary Contact.
[bookmark: _jhrmwqhqep41]Game 03: Inspection Hunt
· Description : A timed 15-minute 3D walkaround drill requiring candidates to locate 100 pre-installed defects across tires, air lines, brake chambers, fifth-wheel coupling, and Tesla diagnostic panels.
· ELDT Mapping : Pre/Post-Trip Inspections, Roadside Inspections.
· Scoring Metrics : Defects Identified (%), Completion Time (min), Critical Safety Misses (Flags).
[bookmark: _kn6bcwr0fg40]Game 04: Load Secure
· Description : Cargo securement puzzle adhering to FMCSA Part 393 standards. Candidates calculate working load limits, place dunnage/straps, adjust weight distribution over axles, and log documentation for a 48,000 lb tractor payload.
· ELDT Mapping : Handling and Documenting Cargo, Environmental Compliance.
· Scoring Metrics : Securement Score (100-pt scale), Axle Weight Compliance, Documentation Accuracy.
[bookmark: _3gdl0fs0kza6]Game 05: Coupling Chaos
· Description : A timed procedural drill for coupling and uncoupling heavy tractor-trailers, including landing gear elevation, glad hand/electrical connection, tug test verification, and Tesla Semi e-coupling activation.
· ELDT Mapping : Coupling and Uncoupling.
· Scoring Metrics : Completion Time (sec), Missed Safety Steps (Flags), Tug Test Verification (Pass/Fail).
[bookmark: _qz2h2q8tewhu]Game 06: HOS Puzzle
· Description : Electronic Logging Device (ELD) simulator where candidates construct compliant shift schedules utilizing 11-hour driving, 14-hour duty, 70-hour/8-day rolling limits, and split sleeper berth provisions.
· ELDT Mapping : Hours of Service (HOS) Requirements.
· Scoring Metrics : Violation-Free Operational Days, Trip Efficiency Rating, Log Audit Accuracy.
[bookmark: _ivjd48di0nm4]Game 07: Hazard Highway
· Description : Dynamic video perception challenge requiring candidates to identify moving hazards (pedestrians, abrupt brake lights, railroad crossing signals, active work zones) within a strict 3-second window.
· ELDT Mapping : Hazard Perception, Railroad-Highway Crossings, Night Operation.
· Scoring Metrics : Hazard Identification Rate (%), Average Response Time (ms), False Positive Rate.
[bookmark: _dt1hgsg9ab6b]Game 08: Skid Recovery
· Description : Emergency maneuver simulator forcing jackknife scenarios, hydroplaning, and regenerative braking loss on slippery surfaces. Candidates practice steering into skids, modulated braking (ABS vs non-ABS), and one-pedal recovery.
· ELDT Mapping : Skid Control / Recovery / Jackknifing, Extreme Driving Conditions.
· Scoring Metrics : Skid Recovery Success (Pass/Fail), Steering Input Smoothness, Stopping Distance Deviation.
[bookmark: _ric51l3c9wa1]Game 09: Tesla Battery Mgmt
· Description : 500-mile long-haul management drill executed from the central driver seat. Candidates balance energy consumption to hit the  1.7 kWh/mi target  while managing battery thermals, elevation grade, regen braking, and 1.2 MW Megacharger stops.
· ELDT Mapping : Maintenance, Vehicle Systems, Environmental Compliance.
· Scoring Metrics : Average Energy Efficiency (kWh/mi), Route Completion Time, Charge Schedule Optimization.
[bookmark: _uelu9lbkaie6]Game 10: Signal Survival Remote CDL
· Description : Teleoperation simulator introducing network disruptions, including  100–400 ms latency , packet drops, and frozen camera streams. Candidates must maintain lane control and trigger emergency stops (e-stop) in <0.8 seconds.
· ELDT Mapping : Distracted Driving, External Communications, Remote Teleoperation Protocol.
· Scoring Metrics : Control Stability During Lag, E-Stop Execution Time (<0.8s target), Signal Recovery Index.
[bookmark: _8esjzvrwpguj]Game 11: Trip Planning Optimizer
· Description : Logistics optimization engine requiring candidates to plot a 500-mile route incorporating Megacharger locations, mandatory HOS rest breaks, weigh station stops, and adverse weather windows.
· ELDT Mapping : Trip Planning, Environmental Compliance.
· Scoring Metrics : On-Time Arrival (%), Total Energy Consumed (kWh), Regulatory Compliance Score.
[bookmark: _5l8z2flodiax]Game 12: Fleet Manager Sim
· Description : Real-Time Strategy (RTS) environment where the candidate oversees 3 remote Tesla Semis simultaneously across 24 video feeds. Requires issuing safety interventions, managing charge queues, and coordinating route re-dirs without direct steering input.
· ELDT Mapping : External Communications, Whistleblower/Coercion.
· Scoring Metrics : Fleet Safety Calls (Accuracy %), Task Completion Efficiency, Teleoperation Downtime.
[bookmark: _6ob7h1trra8i]Game 13: Rescue Relay CDL
· Description : Capstone evaluation scenario simulating a complete highway incident: roadside mechanical fault, scene securement, cargo transfer, and remote dispatch takeover, concluding with a simulated carrier recruitment interview on Day 120.
· ELDT Mapping : Post-Crash Procedures, Identification/Diagnosis of Malfunctions, All Non-Driving Topics.
· Scoring Metrics : Cumulative Safety Score, Incident Resolution Time, Operational Efficiency.
[bookmark: _5tto8efrecaq]Section 6: Scoring Formula, Daily Schedule & Certification Tiers
[bookmark: _w4l1jlt87oo9]Program Scoring Formulas
Candidates receive a composite performance score on every exercise based on a three-part distribution:$$\text{Final Score} = (\text{Accuracy} \times 0.40) + (\text{Efficiency} \times 0.30) + (\text{Safety} \times 0.30)$$
· Accuracy (40%) : Evaluates spatial alignment, placement error (e.g., <10 cm target in backing), task completeness, and regulatory rule adherence.
· Efficiency (30%) : Measures completion speed, route optimization, and Tesla energy economy relative to the baseline target of  1.7 kWh/mile .
· Safety (30%) : Tracks hazard detection latencies, speed limits, mirror check intervals, and flag avoidance.
[bookmark: _xc4a2slf9urf]Experience Points (XP) Calculation
$$\text{XP} = (\text{Accuracy Score} \times 10) + (\text{Efficiency Score} \times 5) - (\text{Safety Flags} \times 50)$$
[bookmark: _jev58rcx0ht1]Daily Instructional Schedule (6-Hour Structure)
+-----------------------------------------------------------------+
|                   DAILY 6-HOUR TRAINING LOOP                    |
+-----------------------------------------------------------------+
| 09:00 - 09:45 | Classroom Micro-Lesson (ELDT Theory Topic)      |
| 09:45 - 12:00 | Game Drills (Maximum of 2 Active Games)         |
| 12:00 - 12:30 | Break / Mid-Day Review                          |
| 12:30 - 14:00 | Ranked Tournament Session (Standardized Seed)  |
| 14:00 - 14:30 | VOD Review & Telemetry Analytics Debrief        |
+-----------------------------------------------------------------+

[bookmark: _i1a07j3p8v1p]Hardware Setup Specifications
· Footprint : Compact commercial-grade motion or static chassis.
· Peripherals : High-torque force feedback wheel, dynamic pedals, multi-position shifter, and dedicated switch panel.
· Tesla Central Seat Mode : Single central seat configuration replicating the Tesla Semi cab layout.
· Displays : Triple-monitor wrap or integrated Virtual Reality (VR) headset for blind-spot scans and backing maneuvers.
· Communications : Noise-canceling headset for remote dispatch communication.
[bookmark: _kw94q4o14pq3]Certification Tiers
  +-------------------------------------------------------------------+
  |                        CERTIFICATION TIERS                        |
  +-------------------------------------------------------------------+
  |  PLATINUM EXPERT  | 10,000+ XP | ELDT TPR + 10h Range / 10h Road   |
  |                   |            | Zero Flags + 1.7 kWh/mi          |
  +-------------------------------------------------------------------+
  |  GOLD             | 5,000 XP   | 85%+ Theory + Signal Survival    |
  +-------------------------------------------------------------------+
  |  SILVER           | 2,000 XP   | 80%+ ELDT Pass + Range Proficient|
  +-------------------------------------------------------------------+
  |  BRONZE           | 500 XP     | 70%+ Clean Completion            |
  +-------------------------------------------------------------------+

· Bronze Tier
· Requirements : Cumulative 500 XP;  70%+ score  on clean completion of initial basic control drills.
· Status : Novice Trainee.
· Silver Tier
· Requirements : Cumulative 2,000 XP;  80%+ theory exam pass score  (FMCSA ELDT standard); verified proficiency on BTW range maneuvers (straight, offset, parallel, alley dock).
· Status : CLP Holder / Range Proficient Operator.
· Gold Tier
· Requirements : Cumulative 5,000 XP;  85%+ overall academic/drill score ; verified pass on Game 10 (Signal Survival Remote CDL) under <250 ms latency parameters; verified Tesla Semi energy economy standard ( 1.7 kWh/mi ).
· Status : Pro League Competitor / Advanced CDL Trainee.
· Platinum Expert CDL Tier
· Requirements : Cumulative 10,000+ XP;  95%+ score  on Game 13 (Rescue Relay Capstone); complete FMCSA ELDT theory verification reported to the Training Provider Registry (TPR);  10 hours Range  and  10 hours Public Road  physically logged;  zero safety flags  recorded during final championship evaluations; maintained target energy efficiency of  1.7 kWh/mi .
· Status : Job-Ready Class A Commercial Driver & Qualified Remote Tesla Semi Teleoperator. Meets all CPUC/FMCSA teleoperation staffing criteria (US CDL, background check, drug/alcohol clearance, and mandatory teleoperation certification).
[bookmark: _q1z6px5lcjxz]Section 7: Developer & Software Integration Specifications
[bookmark: _6ffr7y8eyz7l]Software Architecture Overview
The platform couples an esports tournament software engine operating at hub.esportsleaguehub.com with GoHighLevel (GHL) CRM endpoints to track student progress, issue compliance credentials, and automate carrier hiring pipelines.
[bookmark: _pq18aq69uxzb]Student Profile Payload Schema
{
  "student_profile": {
    "gamertag": "SemiPro_01",
    "ghl_contact_id": "ghl_cnt_88392011",
    "cdl_number": "CDL-CO-9920394-A",
    "program_status": {
      "tier": "Platinum",
      "xp": 10450,
      "season": 4,
      "day_count": 120
    },
    "eldt_compliance": {
      "eldt_theory_pct": 96.5,
      "eldt_status": "Reported_To_TPR",
      "tpr_submission_timestamp": "2026-10-15T23:59:00Z",
      "btw_range_prof": true,
      "btw_range_hours_logged": 12.5,
      "btw_road_prof": true,
      "btw_road_hours_logged": 14.0
    },
    "telemetry_metrics": {
      "tesla_kwhmi": 1.68,
      "estop_reaction_time_sec": 0.62,
      "signal_survival_pass": true
    }
  }
}

[bookmark: _y27v7eqf6xsp]Event Triggers & Webhook Automations
1. Theory Completion Event : Triggers when eldt_theory_pct exceeds 80.0% across all 30 mapped topics. Automatically compiles candidate records for instructor sign-off and transmits data to the FMCSA TPR API.
2. Gold/Platinum Level Up : Updates the GHL contact record stage, applies tag CDL_Remote_Qualified, and triggers SMS/Email notifications to partner motor carrier recruiters.
3. Day 120 Championship Final : Auto-creates an Opportunity stage in GHL titled "Carrier Recruitment Pipeline" containing telemetry fields (tesla_kwhmi, estop_reaction_time_sec, xp) for direct evaluation by fleet hiring managers.

